Name
 GenFds.exe
Synopsis
GenFds.exe [-v | -q | -d] [-w <Workspace>] [-D <Macro=Value>]… [-a <ArchList>] [-o <OutputDir>] [-r <FdName>] [-i <FvName>] [-C <CapsuleImage>] –f <FdfFile> –b <BuildTarget> –t <TagName> –p <PlatformFile>
GenFds.exe –h
GenFds.exe --version
Description
GenFds generates the Ffs, Fv, FD and Section data depending on the selected command line options. It gets the platform, flash and module information from the target.txt, platform.dsc, flashmap.fdf, package.dec and module.inf. The FDF file must be specified and follow the correct FDF specification or the build will stop with an exception
The FDF file describes information about flash parts, as well as rules for combining binaries, (Firmware Image) built from a DSC file. The output of the first phase of an EDK II build (as defined in the EDK II Build Specification) generates valid PE32/PE32+/Coff image files. GenFds performs the second phase of the build process during which consumes the images generated during the first phase, using statements and rules defined in the FDF file to place the PE32/PE32+/Coff images files into one or more EFI sections. The EFI sections may be combined with other optional sections (version, depex, user interface) sections, into EFI Firmware File system (FFS) Sections. FFS images are put into Firmware Volumes (FVs,) and finally, the FV sections are combined into one or more Flash Device binary image (FD.)
The outputDir must be specified. The tool will generate a FV directory which includes a FFS directory, Fv file, Fv INf file and Fd file. The FFS directory contains all modules directory which contains Ffs files and section files. All output of GenFds tool will be in the FV directory. The FV directory structure is as follows. The outputDir should be part of Efi file path. For each of the module described in the FDF file such as the ‘InfFIle’ statement format  the GenFds tool will determing the  input files from the path of  “ $(outputDir)\ $(Arch) \ $(ActivePlatfromName) \$(ModuleName) \$(ModuleName) \DEBUG
1.	If Arch list was specified, the GenFds tool will use this Arch instead of Arch List in Target.txt file
2.	If Workspace was not specified, the GenFds tool will use the Workspace path set in OS environment. 
3.	If ActivePlatform was specified, GenFds tool will use the active platform as the current platform instead of active platform in Target.txt file.
GenFds tool supports 2 kinds of path in command line: Absolute path and relative workspace path. The GenFds tool also supports $(WORKSPACE) marco in path. For example, if the input Fdf is $(WORKSPACE)\NT32PKg\Nt32.fdf, the tool will expand the $(WORKSPACE) macro with real path.
Options
If no options are specified, tool prints error message.
-a,  --arch <ARCHS>
ARCHS is a comma separated (no space) list containing one or more of: IA32, X64, IPF or EBC when built, overrides target.txt’s TARGET_ARCH
-p, --platform PlatformName.dsc
Builds the platform specified by the DSC file name argument, over rides the ACTIVE_PLATFORM
-f, --filename Filename			
Input FDF file and its format must follow FDF specification.
-r, --rom_image FdUiName				
Builds the image using the [FD] section named by FdUiName.
-i, --FvImage UiFvName
	Builds the FV image using the [FV] section named by UiFvName
-C, --CapsuleImage UiCapName
	Build the Capsule image using the [Capsule] section named by UiCapName
-o, --output Dir
The output directory of Genfds tool. This directory also should be the directory of the EFI file.
-w –-workspace
	The current workspace path 
-b --buildtarget DEBUG|RELEASE
Build target is one of: DEBUG, RELEASE.
-t --tagname TOOLCHAIN_TAG
Specifies the tool chain to build the platform.
-D --define MACRO=VALUE
Pass macro to this tool.
-s --specifyaddress ADDRESS
Specifies driver load address.
[--version]
	Print version and copyright of this program and exit
[-v, --verbose]
Enable verbose output with informational messages printed. This is a count value, so specifying –vv can be used to increase the verbosity level.
[-q, --quiet]
	Disable all messages except FATAL ERRORS
[-d, --debug [#]]
	Enable debug messages, at level #
[-h, --help]
	Print copyright, version and usage of this program and exit
Status codes returned
0	The action was completed as requested.	
Nonzero	The action failed.	
Example
1. WORKSAPCE has already set. $(WORKSPACE) = c:\work\EdkII. The Fdf file is in c:\work\EdkII\Nt32pkg\Nt32pkg.fdf. Output directory is c:\work\EdkII\Build\Nt32\Debug_MyTools.  ActivePlatform is C:\work\EdkII\Nt32Pkg\Nt32Pkg.dsc
GenFds –f c:\work\EdkII\Nt32pkg\Nt32pkg.fdf –o c:\work\EdkII\Build\Nt32\Debug_MyTools –p c:\work\EdkII\Nt32pkg\Nt32Pkg.dsc
GenFds –f $(WORKSPACE)\Nt32Pkg\Nt32Pkg.fdf –o $(WORSPACE)\Build\Nt32\Debug_MyTools –p $(WORKSAPCE)\Nt32Pkg\Nt32Pkg.dsc

GenFds –f Nt32Pkg\Nt32Pkg.fdf –o Build\Nt32\Debug_MyTools –p Nt32Pkg\Nt32Pkg.dsc
2. Generate one FD which is defined in FDF file. Use ‘-r’ and Fd UIName. The Fd  UIName is the name which is defined in the FDf file, for detail information refer to FDF specification
GenFds –f GenFds –f c:\work\EdkII\Nt32pkg\Nt32pkg.fdf –o c:\work\EdkII\Build\Nt32\Debug_MyTools –p c:\work\EdkII\Nt32pkg\Nt32Pkg.dsc –r Fv_Recovery
3. Generate one FV which is defined in FDF file. Use ‘-i’ and FV UiName. The FV UIName is the name which is defined in the FDF file, for detail information refers to FDF specification.
GenFds –f c:\work\EdkII\Nt32pkg\Nt32pkg.fdf –o c:\work\EdkII\Build\Nt32\Debug_MyTools –p c:\work\EdkII\Nt32pkg\Nt32Pkg.dsc –I FVRecovery

4. Use command line option to replace the Arch List in Target.txt. 
GenFds –f c:\work\EdkII\Nt32pkg\Nt32pkg.fdf –o c:\work\EdkII\Build\Nt32\Debug_MyTools –p c:\work\EdkII\Nt32pkg\Nt32Pkg.dsc
-a IA32, X64
Bugs
No know issues
Files 
target.txt, platform.dsc, flashmap.fdf, package.dec and module.inf.
See also
 GenFv, GenFfs, GenSection, GenFw.
License
Copyright (c) 1999 - 2011, Intel Corporation. All rights reserved.
This program and the accompanying materials are licensed and made available 
under the terms and conditions of the BSD License which accompanies this 
distribution.  The full text of the license may be found at
http://opensource.org/licenses/bsd-license.php. THE PROGRAM IS DISTRIBUTED UNDER THE BSD LICENSE ON AN "AS IS" BASIS,WITHOUT WARRANTIES OR REPRESENTATIONS OF ANY KIND, EITHER EXPRESS OR IMPLIED.